/****************************************************************************
 * Rage 128 Programmer's Guide Supplement                                   *
 * Video Decoding with the Rage Theatre                                     *
 *                                                                          *
 * Author: Special Projects  1999 07 28                                     *
 *                                                                          *
 * Copyright (c) 1999 ATI Technologies Inc. All rights reserved             *
 ****************************************************************************/

READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT !

ATI Technologies Inc.
33 Commerce Valley Drive East
Thornhill, Ontario
Canada L3T 7N6

Developer Relations Hotline ............ (905) 882-2600 ext. 6000
Developer Relations FAX ................ (905) 944-2655
Developer Relations E-mail ............. devrel@ati.com

Please direct all inquiries about this SDK to Developer Relations at
one of the above two numbers or via the E-mail address.

Head Office, Sales and Marketing ....... (905) 882-2600
Corporate FAX .......................... (905) 882-2620

World Wide Web ......................... http://www.ati.com

*****************************************************************************

RT contains the following example programs:

*****************************************************************************
*    NOTE: No checking is done to see if the monitor supports the           *
*          requested display mode.  Make sure that the monitor              *
*          you are using supports the display mode you are attempting       *
*          to set!                                                          *
*****************************************************************************

*****************************************************************************
*                                                                           *
*    NOTE: All examples in this chapter require an ATI Rage Theater decoder *
*                                                                           *
*****************************************************************************

DECODER.EXE
-detects and initializes the Rage Theatre chip.  The input is selectable, and
video quality (hue, saturation, brightness, contrast) is also adjustable.

KEY     AFFECT
Q       Increase brightness
A       Decrease brightness
W       Increase contrast
S       Decrease contrast
E       Increase saturation
D       Increase saturation
R       Increase hue/tint
F       Decrease hue/tint
X       Toggle sharpness (between smooth and sharp)
SPACE   Reset the video levels to default
T       Increase volume
G       Decrease volume
1       Set input to composite
2       Set input to tuner
3       Set input to Svideo
+       Increase the tuner channel
-       Decrease the tuner channel

CC.EXE
-enables closed captioning capture for the Rage Theatre and Rage 128.  The 2
bytes of closed captioning data are displayed on the screen.

VIP.EXE
-sets up and initializes the VIP subsystem on the Rage 128.  VIP is one of the
protocols used for programming the Rage Theatre.  The VIP device number of the
Rage Theatre, as well as it's device ID and revision are returned, if found.






